JSRDotNETSDK Reference

# InstrumentOpenCriteria Properties

InstrumentOpenCriteria Class See Also

The following tables list the members exposed by the InstrumentOpenCriteria type.

Properties

| Name | Description
--- | --- | ---
| AllowedInterfaces | Gets the list of allowed interface types that can be used by this plugin. The default value for this property is all of the supported interfaces.
| ModelName | The model name of the instrument(s) to be opened, or NULL if any model is acceptable. Examples model names are DPR500, DPR300, PRC50, etc.
| PortsToExclude | If the library is for a family of instruments which connect via serial port, this would be a list of serial port names like COM3. If this list is null or empty, then no ports are excluded in the search for an instrument. For connection types, this may not be used, such as USB.
| PortsToInclude | If the library is for a family of instruments which connect via serial port, this would be a list of serial port names like COM3. If this list is null or empty (the default value), then all ports are included in the search for an instrument. For connection types, this may not be used, such as USB. In a possible future ethernet model, it could be a list of IP address and port numbers, etc.
| SerialNumber | The SerialNumber of the instrument to be opened, or NULL (or alternatively an empty string) if any are acceptable.
| guid | The model name of the instrument(s) to be opened, or NULL if any model is acceptable. Examples model names are DPR500, DPR300, PRC50, etc.

Top
See Also

#### Reference

InstrumentOpenCriteria Class
JSRDotNETSDK Namespace