JSRDotNETSDK Reference

# PulserReceiverImpl.PulserPowerLimitStatus Property

See Also

Gets the current pulser power limit status. Some pulsers can be damaged or suffer a reduction in performance when the combination pulser voltage and pulse repetition frequency is too high. This property returns an integer based on the current settings of the instrument. Some instruments cannot detect the pulse repetition frequency when an external trigger source is used. In this case, this property will return UNKNOWN.

Namespace: JSRDotNETSDK
Assembly: JSRDotNETSDK (in JSRDotNETSDK.dll)
Syntax

VB
C#
C++
JScript
Copy

    [PulserSetting(SettingNames.PulserPowerLimitStatus, PulserPropertyRole.DIRECT, IsVolatile = true)]
    public virtual POWER_LIMIT PulserPowerLimitStatus {get;}

    This language is not supported or no code example is available.

#### Property Value

(enum POWER_LIMIT) The pulser power limit status.

#### Implements

IPulserReceiver.PulserPowerLimitStatus
See Also

#### Reference

PulserReceiverImpl Class
PulserReceiverImpl Members
JSRDotNETSDK Namespace
PulserPowerLimitStatus