JSRDotNETSDK Reference

# IS_PULSING Enumeration

See Also

Values that represent the current activity of the pulser. Some instruments do not have the ability to detect if an external trigger is active or not. However, if the internal trigger source is used, the instrument will report this property as active.

Namespace: JSRDotNETSDK
Assembly: JSRDotNETSDK (in JSRDotNETSDK.dll)
Members

| Member name | Description
--- | --- | ---
| INACTIVE | The pulser trigger circuit is not currently being triggered.
| ACTIVE | The pulser trigger circuit is being currently triggered.
| UNKNOWN | The hardware is unable to report if the pulser is triggered or not.

See Also

#### Reference

JSRDotNETSDK Namespace