JSRDotNETSDK Reference

# PulserReceiverBase.PulserImpedance Property

See Also

Gets or sets the pulser output impedance. Currently only implemented in the DPR300, the LOW_Z option provides a higher pulse energy but with a side effect of lessening the effect of the damping resistor, resulting in less damping. (See the DampingIndex property)

Namespace: JSRDotNETSDK
Assembly: JSRDotNETSDK (in JSRDotNETSDK.dll)
Syntax

VB
C#
C++
JScript
Copy

    [PulserSetting(SettingNames.PulserImpedance, PulserPropertyRole.DIRECT)]
    public abstract PULSER_IMPEDANCE PulserImpedance {get; set;}

    This language is not supported or no code example is available.

#### Property Value

(enum PULSER_IMPEDANCE) The pulser output impedance. (Either High-Z or Low-Z)

#### Implements

IPulserReceiver.PulserImpedance
See Also

#### Reference

PulserReceiverBase Class
PulserReceiverBase Members
JSRDotNETSDK Namespace
PulserImpedance